This code only accepts the trajectory files from output of Yongsheng’s code.

1. Put Trajectories and the referencing (LLE\_ref.csv and xyz\_ref.csv) files in a folder (in this case, the “Trajs” folder) Table

   Description automatically generated
2. Open terminal (anaconda terminal at best, it works as long as you can run python on your terminal)
3. Input: python Georeferencing -i path\_to\_trajs\_folder -o path\_you\_want\_to\_store\_the\_result



1. The result will appear in a folder named “ProcessedTrajs” in your specified output path.

Table

Description automatically generated